Story ID: 
Approach Limits Raised in Canada 
By: Gordon Gilbert
Caption: Responding to recommendations from Canada’s Transportation Safety Board after at least two low-visibility landing accidents, Transport Canada increased the
Word Count: 127
Responding to recommendations from Canada’s Transportation Safety Board after at least two low-visibility landing accidents, Transport Canada increased the minimum visibility required before beginning an approach from the previous 1,200 feet to 1,600 feet, effective December 1. The visibility measurement can be made by a sensor or by a qualified observer if a visibility sensor has not been installed or is out of service. Transport Canada amended the regulations to prohibit commercial operators, including air-taxi services, from beginning an approach under conditions in which a successful landing is unlikely. However, the rule will not apply to operators and crews already approved to lower visibility limits at specified runways. Transport Canada stated that the new rule will help harmonize Canadian regulations with international standards, including those in the U.S.