Story ID: 
FAA: Premier I Software Change Needed
By: Jennifer Harrington
Caption: The FAA has issued AD 2008-16-02 for operators of Premier I (model 390) S/Ns RB-4 through RB-204, which calls for a post-flight residual-heat check of the 
Word Count: 49
The FAA has issued AD 2008-16-02 for operators of Premier I (model 390) S/Ns RB-4 through RB-204, which calls for a post-flight residual-heat check of the angle-of-attack probes after every flight until a software change is made or the probe is replaced. The AD becomes effective on September 3.