Story ID: 
Garmin's G1000 NXi Coming To Piper M500
By: Chad Trautvetter
Caption: STC approval of the G1000 NXi for existing G1000-equipped M500 is slated for next year. The installation requires no panel modifications, Garmin said.
Word Count: 154
The upgraded Garmin G1000 NXi integrated flight deck is headed for the Piper M500. Compared with the turboprop single’s original G1000 avionics, the NXi version adds features such as SurfaceWatch runway monitoring technology and visual approaches.

STC approval of the G1000 NXi for existing G1000-equipped M500s is slated for next year. The installation requires no panel modifications, Garmin said.

Other features available with the NXi include geographical map overlay within the HSI, supporting the display of Nexrad and Flight Information Service-Broadcast (FIS-B) weather, weather radar, SafeTaxi airport diagrams, traffic, and terrain. On the multifunction display, pilots can overlay European visual reporting points on the moving map, as well as sectional and IFR low/high en route charts.

Meanwhile, Flight Stream 510 and Connext technology enables the wireless transfer of aviation databases from the Garmin Pilot app on a mobile device to the G1000 NXi.