Story ID: 046
Gulfstream G700 Program Reaches 1,100-hour Mark
By: Kerry Lynch
Caption: Gulfstream's new flagship G700 remains on track for market entry in late 2022 with certification flight trials anticipated later this year.
Word Count: 627
One year after Gulfstream Aerospace first flew its new G700 flagship, the flight-test program has now accumulated 1,100 flight hours and completed most of the development testing in preparation for certification flight trials, keeping the aircraft on track for market entry in late 2022.

The first flight-test aircraft flew on Feb. 14, 2020, and Colin Miller, Gulfstream senior v-p of innovation, engineering, and flight, told reporters today that the flight-test program “has continued uninterrupted ever since.”

That first aircraft has been used for envelope expansion, reaching as high as 54,000 feet and Mach 0.999. Jake Howard, the lead test pilot for the G700 program, noted the dive speed that Gulfstream must test to for the G700 is Mach 0.995. When asked about potential supersonic testing, he said there was no “intent to intentionally” fly beyond that speed in testing.

In addition to high speed, the aircraft also has performed low-speed and stall tests, including with wing ice shapes. Throughout the flight regime the aircraft has “performed remarkably well, flying virtually squawk free” and is meeting performance expectations, Miller said. Meanwhile, the aircraft’s Rolls-Royce Pearl 700 engines are performing “fantastically well; they are extremely efficient giving us great results for speed, range, and low emissions,” he added.

Gulfstream has since added four more aircraft to the program, with the fifth and final flight-test aircraft flying in late October. In addition, two more aircraft will be dedicated to interior testing and associated supplemental type certificate work. The first of these two, Miller said, is in the late stages of outfitting.

The flight-test program has completed its “initial paces” in field performance testing, demonstrating a full gross-weight balanced field takeoff of about 6,250 feet with a typical landing distance of around 2,500 feet. 

Gulfstream further has flown a G700 to Van Nuys and San Jose, California, as well as Chicago, to support sales and marketing. During those trips, Miller said that the company tested the avionics in a variety of different conditions and approach procedures “proving out the robustness” of the Symmetry flight deck.

The G700 comes with a predictive landing performance system that Miller termed as a breakthrough and said is designed to shield against runway overrun and warns pilots to go around when necessary. The flight trials have further been examining the performance of the new dual HUD that includes enhanced vision system and synthetic vision. The enhanced vision system will be given landing credit down to touchdown and rollout, Miller said.

As for the program schedule, Miller conceded the pandemic may have forced the shifting around a few parts of the test program but that the company has been able to keep the flight tests and lab work on track to keep the program on its intended pace. This has included folding in remote work where possible.

He noted that the program is its first involving development testing to make sure the aircraft performs as expected, especially with new equipment such as the synthetic vision on the HUD. And then it moves on to company testing, which he characterized as the “dress rehearsal” for the certification trials. Miller estimated the program has completed most of the development testing and roughly half of the company testing with certification testing anticipated to begin later this year. “Almost everything on the airplane we’ve looked at least once already.”

The aircraft, the largest in the Gulfstream portfolio with up to five living areas and 20 windows the size of those on the G650, will be certified to fly 7,500 nm and at speeds of Mach 0.925. Miller noted that he discovered that once he flew the aircraft, he immediately forgot how large it was and called it responsive and predictable.