Story ID: 
Nav Canada Issues Guidance on RVSM
By: Gordon Gilbert
Caption: Advanced operational information on the implementation of reduced vertical separation minimum airspace in northern Canada, scheduled to start April 18, is 
Word Count: 65
Advanced operational information on the implementation of reduced vertical separation minimum airspace in northern Canada, scheduled to start April 18, is available from Nav Canada at (613) 562-5678 or online at www@navcanada.ca under “Special Projects.” Canadian RVSM airspace will initially be implemented from 57 deg north latitude to the North Pole encompassing FL 290 to FL 410 inclusive. An RVSM transition area will begin at 52 deg north latitude.