Story ID: 425OnboardSystems
Onboard Systems Debuts New Non-Rotating Cargo Hook
By: Curt Epstein
Caption: The new kit will fit a variety of Bell helicopters and is on track for summer certification.
Word Count: 188
Vancouver, Wa.-based Onboard Systems International is displaying its new non-rotating cargo hook system for the Bell 204, 205, 212 and 412 at Heli-Expo 2015. The suspension system features stainless steel tension straps rather than the cables used on other non-rotating cargo systems, as well as the company’s Talon MC Keeperless Cargo Hook.
  
“We’ve had a number of customer requests for a non-rotating hook for these Bell aircraft over the years,” noted company sales and marketing vice president Karsten Lemmon. “These new cargo hook systems are designed specifically for operators whose external load missions require non-rotating loads such as back-burning, fertilizer spreading and firefighting, to name a few.”
  
The new systems, designed to reduce ongoing maintenance expenses and lifetime cost, will be available in two configurations: with or without an integrated onboard weighing system that allows the pilot to instantly know the cargo weight. The company expects to receive FAA certification in mid-2015, with Transport Canada and EASA approval to follow. Show attendees can view the system at the company’s booth, and register for a chance to win a Microsoft Surface Pro 3 tablet computer.