Story ID: 
RVSM Introduced in Indonesia
By: Gordon Gilbert
Caption: As of November 25, Indonesia implemented reduced vertical separation minimums (RVSM) between FL 350 and FL 390.
Word Count: 35
As of November 25, Indonesia implemented reduced vertical separation minimums (RVSM) between FL 350 and FL 390. After an initial three-month evaluation trial and favorable safety assessment, flight levels possibly will be expanded to include FL 310 to FL 390.