Story ID: 
Toyota experimental single is carbon fiber
By: AIN Staff
Caption: Toyota confirmed that the fuselage of its experimental four-seat piston aircraft is a one-piece co-cured (single-molded) unit of a carbon fiber and resin c
Word Count: 38
Toyota confirmed that the fuselage of its experimental four-seat piston aircraft is a one-piece co-cured (single-molded) unit of a carbon fiber and resin composite material. The aircraft flew for the first time at Mojave (Calif.) Airport on May 31.